4.2 DS400 port

Next: 4.3 The Z80 and Up: 4. Notes on supported Previous: 4.1.3 Bankswitching Contents Index

# 4.2 DS400 port

The DS80C400 microcontroller has a rich set of peripherals. In its built-in ROM library it includes functions to access some of the features, among them is a TCP stack with IP4 and IP6 support. Library headers (currently in beta status) and other files are provided at ftp://ftp.dalsemi.com/pub/tini/ds80c400/c_libraries/sdcc/index.html.