4.6.4 Preprocessor Macros

Next: 4.6.5 Directories Up: 4.6 The PIC16 port Previous: 4.6.3 Environment Variables Contents Index

## 4.6.4 Preprocessor Macros

PIC16 port defines the following preprocessor macros while translating a source.

Macro | Description
SDCC_pic16 | Port identification
__pic16 | Port identification (same as above)
pic18fxxxx | MCU Identification. xxxx is the microcontrol identification number, i.e. 452, 6620, etc
__18Fxxxx | MCU Identification (same as above)
STACK_MODEL_nnn | nnn = SMALL or LARGE respectively according to the stack model used

In addition the following macros are defined when calling assembler:

Macro | Description
__18Fxxxx | MCU Identification. xxxx is the microcontrol identification number, i.e. 452, 6620, etc
SDCC_MODEL_nnn | nnn = SMALL or LARGE respectively according to the memory model used for SDCC
STACK_MODEL_nnn | nnn = SMALL or LARGE respectively according to the stack model used