3.2.1 Processor Selection Options

Next: 3.2.2 Preprocessor Options Up: 3.2 Command Line Options Previous: 3.2 Command Line Options Contents Index

##
3.2.1 Processor Selection Options

- [-mmcs51] Generate code for the Intel MCS51 family of processors. This is the default processor target.
- [-mds390] Generate code for the Dallas DS80C390 processor.
- [-mds400] Generate code for the Dallas DS80C400 processor.
- [-mhc08] Generate code for the Freescale/Motorola HC08 family of processors.
- [-mz80] Generate code for the Zilog Z80 family of processors.
- [-mgbz80] Generate code for the GameBoy Z80 processor (Not actively maintained).
- [-mavr] Generate code for the Atmel AVR processor (Not maintained, not complete). AVR users should probably have a look at winavr http://sourceforge.net/projects/winavr or http://www.avrfreaks.net/index.php?name=PNphpBB2&file=index, which is based on AVR-port of the gcc compiler.

- [-mpic14] Generate code for the Microchip PIC 14-bit processors (p16f84 and variants. In development, not complete).

- [-mpic16] Generate code for the Microchip PIC 16-bit processors (p18f452 and variants. In development, not complete).
- [-mtlcs900h] Generate code for the Toshiba TLCS-900H processor (Not maintained, not complete).
- [-mxa51] Generate code for the Phillips XA51 processor (Not maintained, not complete).

Next: 3.2.2 Preprocessor Options Up: 3.2 Command Line Options Previous: 3.2 Command Line Options Contents Index