4.6.9 Adding New Devices to the Port

Next: 4.6.10 Memory Models Up: 4.6 The PIC16 port Previous: 4.6.8 Libraries Contents Index

## 4.6.9 Adding New Devices to the Port

Adding support for a new 16bit PIC MCU requires the following steps:

1. Create picDEVICE.c and picDEVICE.h from pDEVICE.inc using
   `perl /path/to/sdcc/support/scripts/inc2h-pic16.pl /path/to/gputils/header/pDEVICE.inc`
2. `mv picDEVICE.h /path/to/sdcc/device/include/pic16`
3. `mv picDEVICE.c /path/to/sdcc/device/lib/pic16/libdev`
4. Add DEVICE to `/path/to/sdcc/device/lib/pic16/pics.all`
   Note: No 18f prefix here!
5. Edit `/path/to/sdcc/device/include/pic16/adc.h`
   Add the new devices to the correct ADC style class (depending on the number of ADC channels).
   Do not touch `adc.h` if the device does not offer any ADC at all.
6. Edit `/path/to/sdcc/device/include/pic16/pic18fregs.h`
   The file format is self-explanatory, just add
   `#elif defined(picDEVICE)`
   `# include <picDEVICE.h>`
   at the right place (keep the file sorted, please).
7. Edit `/path/to/sdcc/device/include/pic16devices.txt`
   Copy and modify an existing entry or create a new one and insert it at the correct place (keep the file sorted, please).
8. Add the device to `/path/to/sdcc/device/lib/pic16/libdev/Makefile.am`
   Copy an existing entry and adjust the device name.
9. Add the device to `/path/to/sdcc/device/lib/pic16/libio/Makefile.am`
   Copy the record from the 18f2220 and adjust the device name.
   If the new device does not offer ADC, I C, and/or (E)USART functionality as assumed by the library, remove the lines with references to `adc/*.c`, `usart/*.c`, or `usart/*.c`, respectively.
10. Update `libdev/Makefile.in` and `libio/Makefile.in` using
    `./bootstrap.sh`
    in `/path/to/sdcc/device/lib/pic16`.
11. Recompile the pic16 libraries as described in 4.6.8.

Next: 4.6.10 Memory Models Up: 4.6 The PIC16 port Previous: 4.6.8 Libraries Contents Index