3.2.7 GBZ80 Options

Next: 3.2.8 Optimization Options Up: 3.2 Command Line Options Previous: 3.2.6 Z80 Options Contents Index

##
3.2.7 GBZ80 Options

- [--callee-saves-bc] Force a called function to always save BC.
- [--no-std-crt0] When linking, skip the standard crt0.o object file. You must provide your own crt0.o for your system when linking.
- [-bo <Num>] Use code bank <Num>.
- [-ba <Num>] Use data bank <Num>.
- [--codeseg <Value>] Use <Value> for the code segment name.
- [--constseg <Value>] Use <Value> for the const segment name.